

**GL-NVR6208**

**Specification: Intelligent Video Recorder 10CH 1SATA 4K Smart NVR**

|  |  |
| --- | --- |
| ***Specs & Model No.*** | ***GL-NVR6204*** |
| ***VIDEO*** |
| ***Network video input*** | *10CH* |
| ***Network bandwidth*** | *80Mbps;* |
| ***Video compression*** | *H.264* |
| ***Video output*** | *1 CH VGA output (1920×1080@60HZ,1280×1024@60HZ)* |
| *HD HDMI output (3840×2160@30HZ,1920×1080@60HZ,1280×1024@60HZ)* |
| ***Display mode*** | *Synchronous output* |
| ***System mode*** | *8 digits +9 preview +8 playback* |
| ***Video bitrate*** | *16-16000Kbps* |
| ***Video resolution*** | *4K/5MP/4MP/3MP/1080P/960P/720P/D1/VGA/4CIF/DCIF/2CIF/CIF/QCIF* |
| ***Image display*** | *1/4/6/8/9 image display* |
| ***Snapshot mode*** | *Support timing snapshot, manual snapshot, JPEG format* |
| ***Motion detection*** | *Support 396(22\*18) surveyed area can be set in every screen and multi-level sensitivity adjustable* |
| ***Privacy mask*** | *Support 4 zones* |
| ***intelligent detection*** | *support IPC intelligent functions (Target counting, Object left/lost, Electronic fence, Line crossing, Humanoid detection, Retrograde detection, Off duty detection, Electric vehicle detection)* |
| ***AUDIO*** |
| ***Audio compression*** | *G.711u* |
| ***Audio input/ output*** | *1 CH RCA input/ 1 CH RCA output port (IPC complex audio input)* |
| ***Bidirectional talk***  | *Bidirectional talk, RCA port* |
| ***VIDEO RECORDING AND PLAYBACK*** |
| ***Video frame rate*** | *1-30fps* |
| ***Record mode*** | *manual/Timing record and alarm record/Timing record/alarm record/Stop record* |
| ***Playback ability*** | *Support 1CH 4K/5MP/4MP/3MP; 4CH 1080P; 8CH sub stream sync playback* |
| ***Playback mode*** | *Instant playback, local record, Playback snapshot, external file playback* |
| ***Record search*** | *Time, calendar, channel search, event search, (ANR, regular video, motion detection video, alarm video, intelligent detection video)* |
| ***Video playback*** | *Start time, play/pause, stop, forward, backward, single frame, forward 30 seconds, backward 30 seconds, fast play(1-16X), slow play(1-1/16X), 1/4/9 split screen, previous page, next page, backup, capture, show hidden progress bar, full screen, roller amplification time bar precise playback* |
| ***STORAGE AND BACKUP*** |
| ***Storage interface*** | *1\*SATA, Single max.16 TB* |
| ***Disk grouping & quota*** | *According video channels to set HDD quantity/ According video channels to set HDD storage capacity* |
| ***Backup location*** | *Local, network, IPSAN & USB* |
| ***ANR*** | *According video channels to set HDD quantity* |
| ***FUNCTION*** |
| ***Network protocol*** | *TCP/IP, HTTP, HTTPS, DDNS, SMTP(SSL), DHCP, PPPoE, UPnP, NTP, P2P, ONVIF, RTSP, HTTP, HTTPS, RTMP* |
| ***Mobile surveillance*** | *Support Apple, Android* |
| ***Internet explorer*** | *Support IE, Chrome, Firefox, Safari* |
| ***Display function*** | *Channel shortcuts: modify the channel, 3D positioning, display AI intelligent rules and results, capture, voice intercom, channel audio, manual recording, instant playback, video parameters* |
| *Desktop display: audio input, volume, alarm information (deployment/removal), P2P cloud service, network information, Output adjustment, system information, device list (showing whether IPC is online or not, recording type), organizational structure (custom channel classification for quick preview), channel round tour, 1/4/6/8/9 split screen, open round tour, open linkage preview, file backup, full screen, hide OSD, PTZ control* |
| ***IPC timing*** | *Manual/auto/timing/reconnect timing to IPC timing* |
| ***Alarm linkage*** | *Send email, audible warning (buzzer), alarm on monitor, upload to center, record, snapshot, preview, PTZ linkage* |
| ***Network detection*** | *Flow monitoring, network wireshark, network test* |
| ***User management*** | *User add, delete, modify, permission management, Fslink Scan the QR code to retrieve the password* |
| ***Manage IPC*** | *Modify IPC parameters* |
| ***EXT INTERFACE*** |
| ***Network interface*** | *1\*RJ45 100M1000M adaptive Ethernet port* |
| ***Alarm input/ output*** | *4CH input/ 1CH output* |
| ***RS-485*** | *1CH* |
| ***USB Port*** | *Rear panel:2\*USB2.0* |
| ***GENERAL*** |
| ***Power supply*** | *DC12V/4A,*  *≤10W* *Power consumption (Without HDD)* |
| ***Temperature*** | *-10°C ~ 55°C/10%-90% humidity* |
| ***Dimension(mm)*** | *360(L)x242.4(W)x48(H)mm,*  *Weight:*  *2KG（Without HDD）* |

**

    

Smart265

    

APP

IMS

SLINK

ONVIF

Vehicle Detect

Absent Alarm

Retrograde

Modify Light Mode

Human Detect

**Key Features:**

* ***10 CH full real-time network video access, 1U NVR case***
* ***H.264 decoding, embedded Linux operation system***
* ***Support sync video recording, remote monitoring, backup***
* ***Support VGA/HDMI sync output, support 2160P HD preview***
* ***Support amplification preview and playback video image***
* ***Standard ONVIF G, S & T, RTSP protocol***
* ***Support external alarm, bi-direction talk, alarm snapshot, email sending functions***
* ***Support DDNS, EMAIL, UPNP, NTP, P2P etc.***
* ***Support WEB, mobile viewer, Client***
* ***support IPC intelligent functions (Target counting, Object left/lost, Electronic fence, Line***
* ***crossing, Humanoid detection, Retrograde detection, Off duty detection, Electric vehicle detection)***
* ***Support grouping disk quota, and disk inventory two storage pattern, distribute different video***
* ***storage capacity or cycle according to different channels***
* ***Support IPC centralized management, including IPC parameters configuration, import and export information, information real time acquisition etc.***
* ***Support channel grouping, preview round touring***
* ***Support network detection (network flow monitoring, network wireshark, network clear) function etc.***
* ***Support max 8CH sub stream sync playback and multi-channel sync play backward***
* ***Support instant playback***
* ***The new UI interface, support a key to open the video recording***
* ***Support IP filter***
* ***BIS, CE, FCC, ISO & ROHS Compliance***

**\***[**www.glotecinc.com**](http://www.glotecinc.com/)

 

**\*Product casing and specifications are subject to change without prior notice.**