


***GL-NVR6216***






*GL-NVR6216*

**Key Features:**

* ***Support 8ch 5MP video real-time access, Mini 1U NVR, 1 SATA.***
* ***Support H.265/H.264/MJPEG, embedded Linux operating system.***
* ***Support video playback, remote monitoring and backup.***
* ***Support preview and playback with 12X electronic zoom.***
* ***Standard ONVIF S, G & T, RTSP***
* ***Support DDNS, EMAIL, UPNP, NTP etc.***
* ***Support Web, mobile monitoring, PC client, CMS software.***
* ***Support TUTK P2P***
* ***Support channel grouping, preview cycle.***
* ***Support 10ch D1 video synchronous playback and multi-channel synchronous playback backward.***
* ***Support dual password authentication and zero channel function.***
* ***BIS, CE, ISO, FCC & ROHS Compliance.***

**Specification:**

**APPLICATION EXAMPLE :** 

**10 CH & 1SATA 1U 5MP REALTIME H.265 NVR**

|  |  |  |
| --- | --- | --- |
| ***Specs & Model No.*** | | ***GL-NVR5108*** |
| ***SYSTEM*** | | |
| ***Operating System*** | ***Embedded Linux Operating System*** | |
| ***VIDEO PARAMETER*** | | |
| ***Network Video Input*** | | ***10ch 5MP/3MP/1080p/960p/720p*** |
| ***Network Video Output*** | | ***VGA/HDMI, 1920×1080@60HZ, 1280×1024@60HZ*** |
| ***Video Bitrate*** | | ***16-8000Kbps*** |
| ***Video Input Bandwidth*** | | ***60Mbps*** |
| ***Image Preview*** | | ***1CH 5MP / 4CH 720P / 6CH Big Picture 5MP; Small Picture:720\*567 / 8CH D1*** |
| ***Video Compression*** | | ***H.265/H.264/MJPEG*** |
| ***Capture Mode*** | | ***Schedule/Manual, JPEG format*** |
|  | |  |
| ***AUDIO PARAMETER*** | | |
| ***Audio Output*** | | ***1CH RCA output*** |
| ***Audio Compression*** | | ***G.711A*** |
| ***STORAGE*** | | |
| ***HDD Interface*** | | ***1 SATA interface*** |
| ***Raid Mode*** | | ***N/A*** |
| ***Capacity*** | | ***Support Max. 8TB HDD*** |
| ***ALARM*** | | |
| ***Motion detection*** | | ***Support image set to 396 (22\*18) detection areas, multistage sensitivity*** |
| ***NETWORK MANAGEMENT*** | | |
| ***Network Protocols*** | | ***TCP/IP,HTTP,DDNS,SMTP(SSL),DHCP,PPPOE,UPNP,NTP,P2P,ONVIF*** |
| ***Compliance Protocol*** | | ***ONVIF Profile S, G & T, RTSP*** |
| ***Remote Application*** | | ***WEB(IE, Chrome, Firefox, Safari), iOS, Android Mobile monitor*** |
| ***Others*** | | ***Dual password authentication, 0 Channel*** |
| ***Smart Detection*** | | ***Object Count, Object left/loss, Area Detection, Line crossing (with Smart IPC)*** |
| ***VIDEO MANAGEMENT*** | | |
| ***Record Mode*** | | ***Manual/Schedule record, Motion alarm record, Motion alarm Snap, link down record*** |
| ***Record Frame Rate*** | | ***1-30fps*** |
| ***Video Query*** | | ***Time, Date, Event, Channel, Exact Search (accurate to second)*** |
| ***Record Storage Path*** | | ***Local, Network, NAS, IPSAN*** |
| ***Front Smart Detection*** | | ***Area Detection, Object Left/Loss, Line Crossing, Object Count, Motion Detection*** |
| ***Local Smart Detection*** | | ***N/A*** |
| ***PLAYBACK & BACKUP*** | | |
| ***Playback Mode*** | ***Multi-channel real-time recording, Regular playback, instant replay, event playback, external file playback,1/4/8 Video input (IP)/ Decode 8\*5M/1\*5M Access bandwidth*** | |
| ***Playback Capability*** | ***1ch (5MP/3MP/1080P) / 4ch(720P)*** | |
| ***Playback Operations*** | ***Play, Stop, Forward, Backward, 30s Forward, 30s Backward, Fast play, Slow play, Single frame, Hide/Show the Time Bar, Backup, Screenshot, Full screen selection*** | |
| ***Backup Mode*** | ***Removable HDD, USB flash disk, Network backup*** | |
| ***EXTERNAL INTERFACE*** | | |
| ***Network Interface*** | ***1pcs RJ45 interface (100MEthernet interface )*** | |
| ***Audio Interface*** | ***1pcs RCA output*** | |
| ***USB backup Operator interface*** | ***10-bit true color graphic menu operation, 2PCS 2.0 USB interface (Rear Panel)*** | |
| ***RS485 Interface*** | ***N/A*** | |
| ***Alarm Interface*** | ***N/A*** | |
| ***GENERAL*** | | |
| ***Power Supply*** | | ***12V 2AMP*** |
| ***Power Consumption*** | | ***≤ 10W (Without HDD)*** |
| ***Storage Condition*** | | ***-10°C ~ 55°C / 10%-90%RH*** |
| ***Dimension*** | | ***W255 \* D218 \* H42mm*** |
| ***Weight/pcs*** | | ***2 KG*** |

 Home

[**www.glotecinc.com**](http://www.glotecinc.com/)

**\*Product casing and specifications are subject to change without prior notice.**